**n-Hexan**

**C6H14**

**[110-54-3]**

http://www.merck-chemicals.com/is-bin/intershop.static/WFS/Merck-DE-Site/Merck/de_DE/codes/images/GHS02.gif

http://www.merck-chemicals.com/is-bin/intershop.static/WFS/Merck-DE-Site/Merck/de_DE/codes/images/GHS08.gif**Signalwort: Gefahr**

http://www.merck-chemicals.com/is-bin/intershop.static/WFS/Merck-DE-Site/Merck/de_DE/codes/images/GHS07.gif

http://www.merck-chemicals.com/is-bin/intershop.static/WFS/Merck-DE-Site/Merck/de_DE/codes/images/GHS09.gif

**H-Sätze:**

H225: Flüssigkeit und Dampf leicht entzündbar.  
H304: Kann bei Verschlucken und Eindringen in die Atemwege tödlich sein.  
H361: Kann vermutlich die Fruchtbarkeit beeinträchtigen oder das Kind im Mutterleib schädigen.  
H373: Kann die Organe schädigen bei längerer oder wiederholter Exposition.  
H315: Verursacht Hautreizungen.  
H336: Kann Schläfrigkeit und Benommenheit verursachen.  
H411: Giftig für Wasserorganismen, mit langfristiger Wirkung.

**P-Sätze:**

P210: Von Hitze/Funken/offener Flamme/heißen Oberflächen fernhalten. Nicht rauchen.  
P240: Behälter und zu befüllende Anlage erden.  
P273: Freisetzung in die Umwelt vermeiden.  
P301 + P310: BEI VERSCHLUCKEN: Sofort GIFTINFORMATIONSZENTRUM oder Arzt anrufen.  
P331: KEIN Erbrechen herbeiführen.  
P302 + P352: BEI KONTAKT MIT DER HAUT: Mit viel Wasser und Seife waschen.  
P403 + P235: Kühl an einem gut belüfteten Ort aufbewahren.

Lagerklasse: 3 Entzündliche flüssige Stoffe

WGK: 2 wassergefährdend